DP-K1 Software Release Note

****** Version 1.10 ******

(ADDITIONAL FUNCTION)

1. ARC function

  - The ARC measurement procedure is now easier than the previous version.

       Added ARC grouping function (Flow view)

          See page 53 of DP-K1 SOFTWARE SETTING MANUAL (Ver 1.04) 

  - The ARC measurement is now visually clearer than the previous version.

       Added function that automatically indicates a range of frequency response for the measurement.
       (Flow view) 

          The range of frequency response is automatically set from 1/2 octave below "Start Frequency"
          to 1/2 octave above "Stop Frequency".

  - Parameter adjustment for the measurement is now easier than the previous version.

       Moved the position of "Parameter Setting" button to lower right on the ARC measurement view.    

  - Added indication of ARC measurement completion.     

       Added indication to view remained time to finish ARC measurement.

2. Improved Communications between PC and Unit (DP-K1)

  - Added an easy-to-follow "Connection Settings" wizard to assist with network communication setup.

       See page 60 of DP-K1 SOFTWARE SETTING MANUAL (Ver 1.04)

  - Added "Simple Connection" function to establish communications without performing network settings.

       See page 60 of DP-K1 SOFTWARE SETTING MANUAL (Ver 1.04)


(MODIFICATION)

The following errors were corrected:

1.  On the mute-all window, mute-all "off" is sometimes indictated although the flow view indicates "on" 
    during Unit connection with mute-all "on".

2.  When measuring with "Box-off" on the ARC box, "Box-off" is indicated on the PC screen of the 
    DP-K1 software although the Unit is operating with "Box-on" after measurement.

3.  The following errors may arise when measuring in ARC grouping.

     1) Data of the ARC filter is not copied onto the grouped ARC box. 
 
     2) After a second ARC measurement, the output gets muted.

4.  When an ARC box that has already been measured is grouped to an existing group, the On/Off button on the ARC
    measurement view is displayed as available without measurement data in the existing group.

5.  Operation on ARC view/table does not work normally after pressing Filter Adjustment on the 
    ARC view.

6.  Frequency response indication on the ARC measurement view may not be updated.

7.  When using four outputs with "External Control Setting > Contact Input > Output Channel" selected,
    PC setting software may shut down depending on time when pushing the output channel select button.

8.  When closing setting software after inputing names on flow view, the Caution Message does not pop
    up advising the user to save the name(s).
 
9.  Changing an output name on flow view causes the input name of the same channel number to also be changed.
    
10. When changing equipment names during communications between the PC and the Unit, the names are
    saved onto PC setting file and not to the Unit.

*************************